EGTS protocol validator v.1.0  Copyright JSC "Navigation-information systems", 2011
------------------------------------------------------------------------------------
File: '5.3.1.bin'
Packet data: 
 0100010B006300010001575800010049010000000909225500050100006E1500303230333D22696E7465726E65742E6265656C696E652E72752C6265656C696E652C6265656C696E65220D0A303230343D2239352E3235352E3235352E3235353A38303132220D0A303430343D31EF60


EGTS Transport Layer:
---------------------
  Validating result   - 0 (OK)

  Protocol Version    - 1
  Security Key ID     - 0
  Flags               - 00000001b (0x01)
       Prefix         - 00
       Route          -   0
       Encryption Alg -    00
       Compression    -      0
       Priority       -       01 (high)
  Header Length       - 11
  Header Encoding     - 0
  Frame Data Length   - 99
  Packet ID           - 1
  No route info       -
  Header Check Sum    - 0x57

EGTS Service Layer:
---------------------
  Validating result   - 0 (OK)

  Packet Type         - EGTS_PT_APPDATA
  Service Layer CS    - 0x60EF

    Service Layer Record:
    ---------------------
    Validating Result    - 0 (OK)

    Record Length               - 88
    Record Number               - 1
    Record flags                -     01001001b (0x49)
        Sourse Service On Device    - 0
        Recipient Service On Device -  1
        Group Flag                  -   0
        Record Processing Priority  -    01 (high)
        Time Field Exists           -      0
        Event ID Field Exists       -       0
        Object ID Field Exists      -        1
    Object Identifier           - 1
    Source Service Type         - 9 (EGTS_FIRMWARE_SERVICE) 
    Recipient Service Type      - 9 (EGTS_FIRMWARE_SERVICE) to ST

       Subrecord Data:
       ------------------
       Validating Result   - 150 (Unknown service)

       Subrecord Type      - 34 (EGTS_SR_SERVICE_FULL_DATA)
       Subrecord Length    - 85


-------------------------------------------------------------
Press any key to exit...
